#N canvas 834 0 932 992 10;
#X obj 106 681 dac~;
#X obj 121 16 adc~;
#X floatatom 325 584 5 0 0 0 - - -;
#X obj 394 544 bng 15 250 50 0 empty empty empty 17 7 0 10 -262144
-1 -1;
#X obj 188 664 tgl 15 0 empty empty empty 17 7 0 10 -262144 -1 -1 0
1;
#X obj 257 629 tgl 15 0 empty empty empty 17 7 0 10 -262144 -1 -1 1
1;
#X text 205 661 record loop out;
#X text 358 581 sequencer value;
#X text 413 541 erase bang;
#X floatatom 463 514 5 0 0 0 - - -;
#X obj 205 51 tgl 15 0 empty empty empty 17 7 0 10 -262144 -1 -1 0
1;
#X obj 291 69 tgl 15 0 empty empty empty 17 7 0 10 -262144 -1 -1 0
1;
#X text 221 49 record loops;
#X text 309 68 play on/off;
#X text 279 627 play on/off out;
#X obj 463 116 bng 15 250 50 0 empty empty erase_loops 17 7 0 10 -262144
-1 -1;
#X floatatom 377 94 5 0 0 0 duration_loops - -;
#X obj 120 153 slicerlooper;
#X text 201 -95 SLICER LOOPER - live looper slicer abstraction.;
#X text 525 198 Click the checkbox 'Record loop' to record a loop.
;
#X text 527 224 Click the checkbox 'Play on/off' to toggle play on
or off;
#X text 527 247 Change the value of the 'Duration loops' box to set
the length of the micro loops. the initial length of the macro loop
will be this duration times the counter \, here set to 16 \, hence
1600 ms or 1.6 seconds.;
#X text 527 307 Click 'Erase loops' to erase sound from the looper.
Remember that an eaqual amount of time as the complete loop time is
required for emptying the looper.;
#X text 526 367 Change the sequence of micro loop playback by swapping
the boxes around. Initially set in 'normal' playback \, from top left
to bottom rigth.;
#X text 527 436 Click the bottom toggle boxes to turn randomized playback
manipulations on and off.;
#X text 425 -56 The 'slicerlooper' is a hybrid implementation between
the traditional beat slicing concept and a delay line based loop machine.
The 'slicerlooper' is based on 16 delay lines instead of one. Initially
it records a loop as one segment \, and plays it back in 'proper' sequence.
By rearranging the radio bars \, one can change the order of the micro
loops. Inlets and outlets in connection to the GUI have been added
for convenient inter-patching.;
#X connect 1 0 17 0;
#X connect 10 0 17 1;
#X connect 11 0 17 2;
#X connect 15 0 17 4;
#X connect 16 0 17 3;
#X connect 17 0 0 0;
#X connect 17 0 0 1;
#X connect 17 1 4 0;
#X connect 17 2 5 0;
#X connect 17 3 2 0;
#X connect 17 4 3 0;
#X connect 17 5 9 0;
